X-Git-Url: http://git.rohieb.name/skm-ma-ws1314.git/blobdiff_plain/9d21dccc2fd73cc36a0ea2527608bfd146912497..refs/heads/reviews:/sec-outlook.tex

diff --git a/sec-outlook.tex b/sec-outlook.tex
index 8e3eb6c..798634a 100644
--- a/sec-outlook.tex
+++ b/sec-outlook.tex
@@ -38,7 +38,12 @@ for power and energy from the node named \emph{Device04}. The device first
 acknowledges this request, and, after retrieving the values, sends them back
 to the client. Afterwards, both sides close their streams.
 
-\input{fig-example-xmpp-stream.tex}
+\begin{figure}[h!]
+  \centering
+  \input{fig-example-xmpp-stream.tex}
+  \caption{Example XMPP stream with sensor data (XEP-0323)}
+  \label{fig:examplexmpp}
+\end{figure}
 
 \paragraph{Control (XEP-0325)~\cite{xep0325}} In this document, a way of
 controlling sensor nodes is specified, which allows a client to get and set
