X-Git-Url: http://git.rohieb.name/skm-ma-ws1314.git/blobdiff_plain/cd6ed40d1dc83be550dc941d629663419f7c53e7..3aebd41deecdba7e92d13378f4a30e6103314433:/main.tex

diff --git a/main.tex b/main.tex
index b2681ad..d6257cc 100644
--- a/main.tex
+++ b/main.tex
@@ -8,8 +8,12 @@
 \usepackage[hidelinks=true]{hyperref}
 \usepackage{todonotes}
 \usepackage{tikz}
+\usepackage{enumitem}  % for sparse lists with \setlist
+
 \usetikzlibrary{arrows}
 \urlstyle{sf}
+\setlist[enumerate]{noitemsep}
+\setlist[itemize]{noitemsep}
 
 \newcommand{\pages}[1]{\marginpar{#1 pages}}
 \newcommand{\term}[1]{\emph{#1}}
@@ -34,6 +38,12 @@ how do we talk to our smart home?
 what are the challenges? (interoperability, H2M interface, self-configuration,
 information filtering to prevent information overflow)
 
+In a distributed context like the Internet of Things, devices need to be ready
+to use out of the box. Users often do not want to set up configurations for each
+device they use, and when using several of those devices, it is often not
+reasonable having to configure every single one.
+
+
 %\paragraph{Human-to-Machine Communication:} especiall in the Internet of Things,
 	%Chatty Things need to be accessible for the user and should be easy to talk
 	%to.
@@ -54,7 +64,7 @@ overview to the techniques used in the paper by Klauk and Kirsche
 \input{sec-discussion.tex}
 
 \bibliographystyle{plain}
-\bibliography{biblio}
+{\small \bibliography{biblio}}
 
 \end{document}
 % vim: set ft=tex et ts=2 sw=2 :
