X-Git-Url: http://git.rohieb.name/skm-ma-ws1314.git/blobdiff_plain/d86e1187722a1fc2aeeb59a03e79fb364b4814ba..f0fb3f3f678d8fe10cad4ff3920a60248a93a077:/main.tex

diff --git a/main.tex b/main.tex
index 38eaf82..692256f 100644
--- a/main.tex
+++ b/main.tex
@@ -5,12 +5,17 @@
 \usepackage{color}
 \usepackage{graphicx}
 \usepackage{wrapfig}
-\usepackage{hyperref}
+\usepackage[hidelinks=true]{hyperref}
+\usepackage{todonotes}
+\usepackage{tikz}
+\usepackage{enumitem}  % for sparse lists with \setlist
 
+\usetikzlibrary{arrows}
 \urlstyle{sf}
+\setlist[enumerate]{noitemsep}
+\setlist[itemize]{noitemsep}
 
 \newcommand{\pages}[1]{\marginpar{#1 pages}}
-\newcommand{\todo}[1][]{\textcolor{red}{TODO #1} \\}
 \newcommand{\term}[1]{\emph{#1}}
 \newcommand{\code}[1]{\textsf{#1}}
 
@@ -24,7 +29,7 @@ Masses with XMPP}
 
 %% Introduction
 \section{Introduction}
-\todo
+\todo{asdf}
 \pages{0-1}
 short overview, not too long: what do we want, what are we going to do?
 
@@ -33,6 +38,12 @@ how do we talk to our smart home?
 what are the challenges? (interoperability, H2M interface, self-configuration,
 information filtering to prevent information overflow)
 
+In a distributed context like the Internet of Things, devices need to be ready
+to use out of the box. Users often do not want to set up configurations for each
+device they use, and when using several of those devices, it is often not
+reasonable having to configure every single one.
+
+
 %\paragraph{Human-to-Machine Communication:} especiall in the Internet of Things,
 	%Chatty Things need to be accessible for the user and should be easy to talk
 	%to.
