X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/298693ec7d300de777ce8ba538766114f1b7b90b..c0d013dd1b33bcab1abb0729aa2585f8631fd27f:/docs/wireless.tex

diff --git a/docs/wireless.tex b/docs/wireless.tex
index dd6ec43dd..f1725318f 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -107,7 +107,7 @@ config wifi-device    wifi device name
 config wifi-iface
     option network  the interface you want wifi to bridge with
     option device   wifi0, wifi1, wifi2, wifiN
-    option mode     ap, sta, adhoc, monitor, or wds
+    option mode     ap, sta, adhoc, monitor, mesh, or wds
     option txpower  (deprecated) transmission power in dBm
     option ssid     ssid name
     option bssid    bssid address
@@ -184,6 +184,9 @@ config wifi-iface
             \item \texttt{monitor} \\
                 Monitor mode
 
+	    \item \texttt{mesh} \\
+		Mesh Point mode (802.11s)
+
             \item \texttt{wds} \\
                 WDS point-to-point link
 
@@ -229,6 +232,11 @@ config wifi-iface
 
 \end{itemize}
 
+\paragraph{Mesh Point}
+
+Mesh Point (802.11s) is only supported by some mac80211 drivers. It requires the iw package
+to be installed to setup mesh links. OpenWrt creates mshN mesh point interfaces.
+
 \paragraph{Wireless Distribution System}
 
 WDS is a non-standard mode which will be working between two Broadcom devices for instance
