X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/61646d6b090ff730f3ccbb3cb3180c9ab6d213f8..5c56c7216aa8f3ad2d9fe92e03ad21278bac5caa:/docs/network.tex?ds=inline

diff --git a/docs/network.tex b/docs/network.tex
index c7e80c68f..e4efd8df9 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -1,4 +1,4 @@
-The network configuration in Kamikaze is stored in \texttt{/etc/config/network}
+The network configuration is stored in \texttt{/etc/config/network}
 and is divided into interface configurations.
 Each interface configuration either refers directly to an ethernet/wifi
 interface (\texttt{eth0}, \texttt{wl0}, ..) or to a bridge containing multiple interfaces.
@@ -169,7 +169,6 @@ config 6tunnel
         option remoteip4        '1.0.0.1'
         option localip4         '1.0.0.2'
         option localip6         '2001::DEAD::BEEF::1'
-        option prefix           '/64'
 \end{Verbatim}
 
 \begin{itemize}
@@ -184,8 +183,6 @@ config 6tunnel
     \item{\texttt{'localip6'}:}
 	IPv6 address to setup on your tunnel side
 	This address is given by the tunnel broker
-    \item{\texttt{'prefix'}:}
-	IPv6 prefix to setup on the LAN.
 \end{itemize}
 
 Using the same package you can also setup an IPv6 bridged connection :
