X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/6fc7a5463c3eaf1c56036b8026dd3672a20ed814..4f5179175e1f15bbc3389f0f7aaa094246c4aad2:/docs/wireless.tex

diff --git a/docs/wireless.tex b/docs/wireless.tex
index d92fa76cd..efb07eafb 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -117,10 +117,13 @@ config wifi-iface
     option key2     key 2
     option key3     key 3
     option key4     key 4
+    option passphrase 0,1
     option server   ip address
     option port     port
     option hidden   0,1
     option isolate  0,1	(broadcom)
+    option doth     0,1	(atheros, broadcom)
+    option wmm      0,1	(atheros, broadcom)
 \end{Verbatim}
 
 \paragraph{Options for the \texttt{wifi-device}:}
@@ -217,6 +220,13 @@ config wifi-iface
     \item \texttt{key, key1, key2, key3, key4} (wep, wpa and psk) \\
         WEP key, WPA key (PSK mode) or the RADIUS shared secret (WPA RADIUS mode)
 
+    \item \texttt{passphrase} (wpa) \\
+        0 treats the wpa psk as a text passphrase; 1 treats wpa psk as
+        encoded passphrase. You can generate an encoded passphrase with
+        the wpa\_passphrase utility. This is especially useful if your
+        passphrase contains special characters. This option only works
+        when using mac80211 or atheros type devices.
+
     \item \texttt{server} (wpa) \\
         The RADIUS server ip address
 
@@ -230,6 +240,14 @@ config wifi-iface
         Optional: Isolation is a mode usually set on hotspots that limits the clients to communicate only with the AP and not with other wireless clients.
         0 disables ap isolation (default); 1 enables ap isolation.
 
+    \item \texttt{doth} \\
+        Optional: Toggle 802.11h mode.
+        0 disables 802.11h (default); 1 enables it.
+
+    \item \texttt{wmm} \\
+        Optional: Toggle 802.11e mode.
+        0 disables 802.11e (default); 1 enables it.
+
 \end{itemize}
 
 \paragraph{Mesh Point}
