X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/8aab380dded91464d39d1ad1221b75d8a50ed539..537ae0547deccf9e7fbae709e2018e3ac82e3c94:/docs/network.tex

diff --git a/docs/network.tex b/docs/network.tex
index 16e5571ae..793a39822 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -22,7 +22,12 @@ of interfaces and add:
 \end{Verbatim}
 
 It is possible to use VLAN tagging on an interface simply by adding the VLAN IDs
-to it, e.g. \texttt{eth0.1}. These can be nested as well.
+to it, e.g. \texttt{eth0.1}. These can be nested as well. See the switch section for
+this.
+
+\begin{Verbatim}
+config inter
+\end{Verbatim}
 
 This sets up a simple static configuration for \texttt{eth0}. \texttt{proto} specifies the
 protocol used for the interface. The default image usually provides \texttt{'none'}
@@ -31,9 +36,27 @@ packages.
 
 When using the \texttt{'static'} method like in the example, the  options \texttt{ipaddr} and
 \texttt{netmask} are mandatory, while \texttt{gateway} and \texttt{dns} are optional.
+You can specify more than one DNS server, separated with spaces:
+
+\begin{Verbatim}
+config interface     "lan"
+    option ifname    "eth0"
+    option proto     "static"
+    ...
+    option dns       "192.168.1.254 192.168.1.253" (optional)
+\end{Verbatim}
+
 DHCP currently only accepts \texttt{ipaddr} (IP address to request from the server)
 and \texttt{hostname} (client hostname identify as) - both are optional.
 
+\begin{Verbatim}
+config interface     "lan"
+    option ifname    "eth0"
+    option proto     "dhcp"
+    option ipaddr    "192.168.1.1" (optional)
+    option hostname  "openwrt"	(optional)
+\end{Verbatim}
+
 PPP based protocols (\texttt{pppoe}, \texttt{pptp}, ...) accept these options:
 \begin{itemize}
     \item{username} \\
@@ -53,6 +76,16 @@ PPP based protocols (\texttt{pppoe}, \texttt{pptp}, ...) accept these options:
 \end{itemize}
 
 For all protocol types, you can also specify the MTU by using the \texttt{mtu} option.
+A sample PPPoE config would look like this:
+
+\begin{Verbatim}
+config interface     "lan"
+    option ifname    "eth0"
+    option proto     "pppoe"
+    option username  "username"
+    option password  "openwrt"
+    option mtu	     1492 (optional)
+\end{Verbatim}
 
 \subsubsection{Setting up static routes}
 
@@ -112,3 +145,66 @@ config switch       "eth0"
     option vlan1    "0 5"
     option vlan2    "4 5"
 \end{Verbatim}
+
+Three interfaces will be automatically created using this switch layout :
+\texttt{eth0.0} (vlan0), \texttt{eth0.1} (vlan1) and \texttt{eth0.2} (vlan2).
+You can then assign those interfaces to a custom network configuration name
+like \texttt{lan}, \texttt{wan} or \texttt{dmz} for instance.
+
+\subsubsection{Setting up IPv6 connectivity}
+
+OpenWrt supports IPv6 connectivity using PPP, Tunnel brokers or static
+assignment.
+
+If you use PPP, IPv6 will be setup using IP6CP and there is nothing to
+configure.
+
+To setup an IPv6 tunnel to a tunnel broker, you can install the
+\texttt{6scripts} package and edit the \texttt{/etc/config/6tunnel}
+file and change the settings accordingly :
+
+\begin{Verbatim}
+config 6tunnel
+        option tnlifname     'sixbone'
+        option remoteip4        '1.0.0.1'
+        option localip4         '1.0.0.2'
+        option localip6         '2001::DEAD::BEEF::1'
+\end{Verbatim}
+
+\begin{itemize}
+    \item{\texttt{'tnlifname'}:}
+        Set the interface name of the IPv6 in IPv4 tunnel
+    \item{\texttt{'remoteip4'}:}
+        IP address of the remote end to establish the 6in4 tunnel.
+	This address is given by the tunnel broker
+    \item{\texttt{'localip4'}:}
+	IP address of your router to establish the 6in4 tunnel.
+	It will usually match your WAN IP address.
+    \item{\texttt{'localip6'}:}
+	IPv6 address to setup on your tunnel side
+	This address is given by the tunnel broker
+\end{itemize}
+
+Using the same package you can also setup an IPv6 bridged connection :
+
+\begin{Verbatim}
+config 6bridge
+	option bridge	'br6'
+\end{Verbatim}
+
+By default the script bridges the WAN interface with the LAN interface
+and uses ebtables to filter anything that is not IPv6 on the bridge.
+This configuration is particularly useful if your router is not
+IPv6 ND proxy capable (see: http://www.rfc-archive.org/getrfc.php?rfc=4389).
+
+
+IPv6 static addressing is also supported using a similar setup as
+IPv4 but with the \texttt{ip6} prefixing (when applicable).
+
+\begin{Verbatim}
+config interface     "lan"
+    option ifname    "eth0"
+    option proto     "static"
+    option ip6addr    "fe80::200:ff:fe00:0/64"
+    option ip6gw     "2001::DEAF:BEE:1"
+\end{Verbatim}
