X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/b9883aef07a63590217f00afe74f586c8ea78e26..31c95ff1eb4ffaeb81f95e959c503904299ab256:/docs/adding.tex

diff --git a/docs/adding.tex b/docs/adding.tex
index 7e6d7abfa..97547ac85 100644
--- a/docs/adding.tex
+++ b/docs/adding.tex
@@ -1,57 +1,111 @@
-Linux is now one of the most widespread operating system for embedded devices due to its openess as well as the wide variety of platforms it can run on. Many manufacturer actually use it in firmware you can find on many devices : DVB-T decoders, routers, print servers, DVD players ... Most of the time the stock firmware is not really open to the consumer, even if it uses open source software.
-
-You might be interested in running a Linux based firmware for your router for various reasons : extending the use of a network protocol (such as IPv6), having new features, new piece of software inside, or for security reasons. A fully open-source firmware is de-facto needed for such applications, since you want to be free to use this or that version of a particular reason, be able to correct a particular bug. Few manufacturers do ship their routers with a Sample Developpment Kit, that would allow you to create your own and custom firmware and most of the time, when they do, you will most likely not be able to complete the firmware creation process.
-
-This is one of the reasons why OpenWrt and other firmware exists : providing a version independent, and tools independent firmware, that can be run on various platforms, known to be running Linux originaly.
-
-\subsection{Which Operating System does this device run ?}
-
-There is a lot of methods to ensure your device is running Linux. Some of them do need your router to be unscrewed and open, some can be done by probing the device using its external network interfaces.
+Linux is now one of the most widespread operating system for embedded devices due
+to its openess as well as the wide variety of platforms it can run on. Many
+manufacturer actually use it in firmware you can find on many devices: DVB-T 
+decoders, routers, print servers, DVD players ... Most of the time the stock 
+firmware is not really open to the consumer, even if it uses open source software.
+
+You might be interested in running a Linux based firmware for your router for
+various reasons: extending the use of a network protocol (such as IPv6), having
+new features, new piece of software inside, or for security reasons. A fully 
+open-source firmware is de-facto needed for such applications, since you want to
+be free to use this or that version of a particular reason, be able to correct a
+particular bug. Few manufacturers do ship their routers with a Sample Development Kit,
+that would allow you to create your own and custom firmware and most of the time,
+when they do, you will most likely not be able to complete the firmware creation process.
+
+This is one of the reasons why OpenWrt and other firmware exists: providing a 
+version independent, and tools independent firmware, that can be run on various 
+platforms, known to be running Linux originally.
+
+\subsection{Which Operating System does this device run?}
+
+There is a lot of methods to ensure your device is running Linux. Some of them do
+need your router to be unscrewed and open, some can be done by probing the device
+using its external network interfaces.
 
 \subsubsection{Operating System fingerprinting and port scanning}
 
-A large bunch of tools over the Internet exists in order to let you do OS fingerprinting, we will show here an example using \textbf{nmap} :
+A large bunch of tools over the Internet exists in order to let you do OS 
+fingerprinting, we will show here an example using \textbf{nmap}:
 
 \begin{Verbatim}
 nmap -P0 -O <IP address>
-Not shown: 1694 closed ports
-PORT     STATE SERVICE
-631/tcp  open  ipp
-1033/tcp open  netinfo
-6000/tcp open  X11
-Device type: general purpose
-Running: Apple Mac OS X 10.4.X
-OS details: Apple Mac OS X 10.4.8 (Tiger)
+Starting Nmap 4.20 ( http://insecure.org ) at 2007-01-08 11:05 CET
+Interesting ports on 192.168.2.1:
+Not shown: 1693 closed ports
+PORT   STATE SERVICE
+22/tcp open  ssh
+23/tcp open  telnet
+53/tcp open  domain
+80/tcp open  http
+MAC Address: 00:13:xx:xx:xx:xx (Cisco-Linksys)
+Device type: broadband router
+Running: Linksys embedded
+OS details: Linksys WRT54GS v4 running OpenWrt w/Linux kernel 2.4.30
+Network Distance: 1 hop
 \end{Verbatim}
 
-nmap is able to report whether your device uses a Linux TCP/IP stack, and if so, will show you which Linux kernel version is probably runs. This report is quite reliable and it can make the distinction between BSD and Linux TCP/IP stacks and others.
+nmap is able to report whether your device uses a Linux TCP/IP stack, and if so,
+will show you which Linux kernel version is probably runs. This report is quite 
+reliable and it can make the distinction between BSD and Linux TCP/IP stacks and others.
 
-Using the same tool, you can also do port scanning and service version discovery. For instance, the following command will report which IP-based services are running on the device, and which version of the service is being used :
+Using the same tool, you can also do port scanning and service version discovery.
+For instance, the following command will report which IP-based services are running
+on the device, and which version of the service is being used:
 
 \begin{verbatim}
 nmap -P0 -sV <IP address>
-
+Starting Nmap 4.20 ( http://insecure.org ) at 2007-01-08 11:06 CET
+Interesting ports on 192.168.2.1:
+Not shown: 1693 closed ports
+PORT   STATE SERVICE VERSION
+22/tcp open  ssh     Dropbear sshd 0.48 (protocol 2.0)
+23/tcp open  telnet  Busybox telnetd
+53/tcp open  domain  ISC Bind dnsmasq-2.35
+80/tcp open  http    OpenWrt BusyBox httpd
+MAC Address: 00:13:xx:xx:xx:xx (Cisco-Linksys)
+Service Info: Device: WAP
 \end{verbatim}
 
-The web server version, if identified, can be determining in knowing the Operating System. For instance, the \textbf{BOA} web server is typical from devices running an open-source Unix or Unix-like.
+The web server version, if identified, can be determining in knowing the Operating
+System. For instance, the \textbf{BOA} web server is typical from devices running 
+an open-source Unix or Unix-like.
 
 \subsubsection{Wireless Communications Fingerprinting}
 
-Although this method is not really known and widespread, using a wireless scanner to discover which OS your router or Access Point run can be used. We do not have a clear example of how this could be achieved, but you will have to monitor raw 802.11 frames and compare them to a very similar device running a Linux based firmware.
+Although this method is not really known and widespread, using a wireless scanner 
+to discover which OS your router or Access Point run can be used. We do not have
+a clear example of how this could be achieved, but you will have to monitor raw 
+802.11 frames and compare them to a very similar device running a Linux based firmware.
 
 \subsubsection{Web server security exploits}
 
-The Linksys WRT54G was originally hacked by using a "ping bug" discoverd in the web interface. This tip has not been fixed for months by Linksys, allowing people to enable the "boot\_wait" helper process via the web interface. Many web servers used in firmwares are open source web server, thus allowing the code to be audited to find an exploit. Once you know the web server version that runs on your device, by using \textbf{nmap -sV} or so, you might be interested in using exploits to reach shell access on your device.
+The Linksys WRT54G was originally hacked by using a "ping bug" discovered in the 
+web interface. This tip has not been fixed for months by Linksys, allowing people
+to enable the "boot\_wait" helper process via the web interface. Many web servers
+used in firmwares are open source web server, thus allowing the code to be audited
+to find an exploit. Once you know the web server version that runs on your device,
+by using \textbf{nmap -sV} or so, you might be interested in using exploits to reach 
+shell access on your device.
 
 \subsubsection{Native Telnet/SSH access}
 
-Some firmwares might have restricted or unrestricted Telnet/SSH access, if so, try to log in with the web interface login/password and see if you can type in some commands. This is actually the case for some Broadcom BCM963xx based firmwares such as the one in Neuf/Cegetel ISP routers, Club-Internet ISP CI-Box and many others. Some commands, like \textbf{cat} might be left here and be used to determine the Linux kernel version.
+Some firmwares might have restricted or unrestricted Telnet/SSH access, if so,
+try to log in with the web interface login/password and see if you can type in 
+some commands. This is actually the case for some Broadcom BCM963xx based firmwares
+such as the one in Neuf/Cegetel ISP routers, Club-Internet ISP CI-Box and many 
+others. Some commands, like \textbf{cat} might be left here and be used to 
+determine the Linux kernel version.
 
 \subsubsection{Analysing a binary firmware image}
 
-You are very likely to find a firmware binary image on the manufacturer website, even if your device runs a proprietary operating system. If so, you can download it and use an hexadecimal editor to find printable words such as \textbf{vmlinux}, \textbf{linux}, \textbf{ramdisk}, \textbf{mtd} and others.
+You are very likely to find a firmware binary image on the manufacturer website,
+even if your device runs a proprietary operating system. If so, you can download
+it and use an hexadecimal editor to find printable words such as \textbf{vmlinux},
+\textbf{linux}, \textbf{ramdisk}, \textbf{mtd} and others.
 
-Some Unix tools like \textbf{hexdump} or \textbf{strings} can be used to analyse the firmware. Below there is an example with a binary firmware found other the Internet :
+Some Unix tools like \textbf{hexdump} or \textbf{strings} can be used to analyse 
+the firmware. Below there is an example with a binary firmware found other the Internet:
 
 \begin{verbatim}
 hexdump -C <binary image.extension> | less (more)
@@ -67,58 +121,78 @@ Scroll over the firmware to find printable words that can be significant.
 
 \subsubsection{Amount of flash memory}
 
-Linux can hardly fit in a 2MB flash device, once you have open the device and located the flash chip, try to find other the Internet its characteristics. If your flash chip is a 2MB or less device, your device is most likely to run a proprietary OS such as Windriver VxWorks, or a custom manufacturer OS like Zyxel ZynOS.
+Linux can hardly fit in a 2MB flash device, once you have opened the device and 
+located the flash chip, try to find its characteristics on the Internet. If
+your flash chip is a 2MB or less device, your device is most likely to run a 
+proprietary OS such as WindRiver VxWorks, or a custom manufacturer OS like Zyxel ZynOS.
 
-OpenWrt does not currently run on devices which have equal or less than 2MB of flash memory. This limitation will probably not be worked around since those devices are most of the time micro routers, or Wireless Access Points, which are not the main OpenWrt target.
+OpenWrt does not currently run on devices which have 2MB or less of flash memory.
+This limitation will probably not be worked around since those devices are most 
+of the time micro-routers, or Wireless Access Points, which are not the main 
+OpenWrt target.
 
 \subsubsection{Pluging a serial port}
 
-By using a serial port, you may reach the console that is being shown by the device for debugging or flashing purposes. By analysing the output of this device, you can easily notice if the device uses a Linux kenrel or something different.
+By using a serial port and a level shifter, you may reach the console that is being shown by the device
+for debugging or flashing purposes. By analysing the output of this device, you can
+easily notice if the device uses a Linux kernel or something different.
 
 \subsection{Finding and using the manufacturer SDK}
 
-Once you are sure your device run a Linux based firmware, you will be able to start hacking on it. If the manufacturer respect the GPL, it will have release with the device, a Sample Developpment Kit.
+Once you are sure your device run a Linux based firmware, you will be able to start
+hacking on it. If the manufacturer respected the GPL, it will have released a Sample
+Development Kit with the device.
 
 \subsubsection{GPL violations}
 
-Some manufacturers do release a Linux based binary firmware, with no sources at all. The first step before doing anything is to read the license coming with your device, then write them about this lack of Open Source code. If the manufacturer answers you they do not have to release a SDK containing Open Source software, then we recommend you get in touch with the gpl-violations.org community.
+Some manufacturers do release a Linux based binary firmware, with no sources at all.
+The first step before doing anything is to read the license coming with your device,
+then write them about this lack of Open Source code. If the manufacturer answers
+you they do not have to release a SDK containing Open Source software, then we 
+recommend you get in touch with the gpl-violations.org community.
 
-You will find below a sample letter that can be sent to the manufacturer :
+You will find below a sample letter that can be sent to the manufacturer:
 
 \begin{verse}
 Miss, Mister,
 
-I am using a <device name>, and I cannot find neither on your website nor on the CD-ROM the open source software used to build or modify the firmware.
+I am using a <device name>, and I cannot find neither on your website nor on the 
+CD-ROM the open source software used to build or modify the firmware.
 
-In conformance to the GPL license, you have to release the following sources :
+In conformance to the GPL license, you have to release the following sources:
 
-- complete toolchain that made the kernel and applications be compiled (gcc, binutils, libc)
-- tools to build a custom firmware (mksquashfs, mkcramfs ...)
-- kernel sources with patches to make it run on this specific hardware, this does not include binary drivers
+\begin{itemize}
+\item complete toolchain that made the kernel and applications be compiled (gcc, binutils, libc)
+\item tools to build a custom firmware (mksquashfs, mkcramfs ...)
+\item kernel sources with patches to make it run on this specific hardware, this does not include binary drivers
+\end{itemize}
 
 Thank you very much in advance for your answer.
 
-Best regards, <your namne>
+Best regards, <your name>
 \end{verse}
 
 \subsubsection{Using the SDK}
 
-Once the SDK is available, you are most likely not to be able to build a complete or functionnal firmware using it, but parts of it, like only the kernel, or only the root filesystem. Most manufacturers do not really care releasing a tool that do work every time you uncompress and use it.
+Once the SDK is available, you are most likely not to be able to build a complete
+or functional firmware using it, but parts of it, like only the kernel, or only
+the root filesystem. Most manufacturers do not really care releasing a tool that
+do work every time you uncompress and use it.
 
-You should anyway be able to use the following components :
+You should anyway be able to use the following components:
 
 \begin{itemize}
-\item kernel sources with more or less functionnal patches for your hardware
+\item kernel sources with more or less functional patches for your hardware
 \item binary drivers linked or to be linked with the shipped kernel version
-\item packages of the toolchain used to compile the whole firmware : gcc, binutils, libc or uClibc
+\item packages of the toolchain used to compile the whole firmware: gcc, binutils, libc or uClibc
 \item binary tools to create a valid firmware image
 \end{itemize}
 
-Your work is now divided into the following tasks :
+Your work can be divided into the following tasks:
 
 \begin{itemize}
 \item create a clean patch of the hardware specific part of the linux kernel
-\item spot potential kernel GPL violations especially on firewall and USB stack stuff
+\item spot potential kernel GPL violations especially on netfilter and USB stack stuff
 \item make the binary drivers work, until there are open source drivers
 \item use standard a GNU toolchain to make working executables
 \item understand and write open source tools to generate a valid firmware image
@@ -126,9 +200,16 @@ Your work is now divided into the following tasks :
 
 \subsubsection{Creating a hardware specific kernel patch}
 
-Most of the time, the kernel source that comes along with the SDK is not really clean, and is not a standard Linux version, it also has architecture specific fixes backported from the \textbf{CVS} or the \textbf{git} repository of the kernel developpment trees. Anyway, some parts can be easily isolated and used as a good start to make a vanilla kernel work your hardware.
+Most of the time, the kernel source that comes along with the SDK is not really 
+clean, and is not a standard Linux version, it also has architecture specific 
+fixes backported from the \textbf{CVS} or the \textbf{git} repository of the 
+kernel development trees. Anyway, some parts can be easily isolated and used as 
+a good start to make a vanilla kernel work your hardware.
 
-Some directories are very likely to have local modifications needed to make your hardware be recognized and used under Linux. First of all, you need to find out the linux kernel version that is used by your hardware, this can be found by editing the \textbf{linux/Makefile} file.
+Some directories are very likely to have local modifications needed to make your
+hardware be recognized and used under Linux. First of all, you need to find out 
+the linux kernel version that is used by your hardware, this can be found by 
+editing the \textbf{linux/Makefile} file.
 
 \begin{verbatim}
 head -5 linux-2.x.x/Makefile
@@ -136,12 +217,14 @@ VERSION = 2
 PATCHLEVEL = x
 SUBLEVEL = y
 EXTRAVERSION = z
-NAME=Avast! A bilge rat!
+NAME=A fancy name
 \end{verbatim}
 
-So now, you know that you have to download a standard kernel tarball at \textbf{kernel.org} that matches the version being used by your hardware.
+So now, you know that you have to download a standard kernel tarball at 
+\textbf{kernel.org} that matches the version being used by your hardware.
 
-Then you can create a \textbf{diff} file between the two trees, especially for the following directories :
+Then you can create a \textbf{diff} file between the two trees, especially for the 
+following directories:
 
 \begin{verbatim}
 diff -urN linux-2.x.x/arch/<sub architecture> linux-2.x.x-modified/arch/<sub architecture> > 01-architecture.patch
@@ -149,29 +232,85 @@ diff -urN linux-2.x.x/include/ linux-2.x.x-modified/include > 02-includes.patch
 diff -urN linux-2.x.x/drivers/ linux-2.x.x-modified/drivers > 03-drivers.patch
 \end{verbatim}
 
-This will constitute a basic set of three patches that are very likely to contain any needed modifications that has been made to the stock Linux kernel to run on your specific device. Of course, the content produced by the \textbf{diff -urN} may not always be relevant, so that you have to clean up those patches to only let the "must have" code into them.
+This will constitute a basic set of three patches that are very likely to contain
+any needed modifications that has been made to the stock Linux kernel to run on 
+your specific device. Of course, the content produced by the \textbf{diff -urN} 
+may not always be relevant, so that you have to clean up those patches to only 
+let the "must have" code into them.
+
+The first patch will contain all the code that is needed by the board to be 
+initialized at startup, as well as processor detection and other boot time 
+specific fixes.
+
+The second patch will contain all useful definitions for that board: addresses, 
+kernel granularity, redefinitions, processor family and features ...
+
+The third patch may contain drivers for: serial console, ethernet NIC, wireless 
+NIC, USB NIC ... Most of the time this patch contains nothing else than "glue"
+code that has been added to make the binary driver work with the Linux kernel. 
+This code might not be useful if you plan on writing drivers from scratch for 
+this hardware.
 
-The fist patch will contain all the code that is needed by the board to be initialized at startup, as well as processor detection and other boot time specific fixes.
+\subsubsection{Using the device bootloader}
 
-The second patch will contain all useful definitions for that board : adresses, kernel granularity, redifinitions, processor family and features ...
+The bootloader is the first program that is started right after your device has 
+been powered on. This program, can be more or less sophisticated, some do let you 
+do network booting, USB mass storage booting ... The bootloader is device and 
+architecture specific, some bootloaders were designed to be universal such as 
+RedBoot or U-Boot so that you can meet those loaders on totally different 
+platforms and expect them to behave the same way.
 
-The third patch may contain drivers for : serial console, ethernet NIC, wireless NIC, USB NIC ... Most of the time this patch contains nothing else than "glue" code that has been added to make the binary driver work with the Linux kernel. This code might not be useful if you plan on writing from scratch drivers for this hardware.
+If your device runs a proprietary operating system, you are very likely to deal 
+with a proprietary boot loader as well. This may not always be a limitation, 
+some proprietary bootloaders can even have source code available (i.e : Broadcom CFE).
+
+According to the bootloader features, hacking on the device will be more or less 
+easier. It is very probable that the bootloader, even exotic and rare, has a 
+documentation somewhere over the Internet. In order to know what will be possible 
+with your bootloader and the way you are going to hack the device, look over the 
+following features :
+
+\begin{itemize}
+\item does the bootloader allow net booting via bootp/DHCP/NFS or tftp
+\item does the bootloader accept loading ELF binaries ?
+\item does the bootloader have a kernel/firmware size limitation ?
+\item does the bootloader expect a firmware format to be loaded with ?
+\item are the loaded files executed from RAM or flash ?
+\end{itemize}
+
+Net booting is something very convenient, because you will only have to set up network
+booting servers on your development station, and keep the original firmware on the device
+till you are sure you can replace it. This also prevents your device from being flashed,
+and potentially bricked every time you want to test a modification on the kernel/filesystem.
+
+If your device needs to be flashed every time you load a firmware, the bootlader might
+only accept a specific firmware format to be loaded, so that you will have to 
+understand the firmware format as well.
 
 \subsubsection{Making binary drivers work}
 
-As we have explained before, manufacturers do release binary drivers in their GPL tarball. When those drivers are statically linked into the kernel, they become GPL as well, fortunately or unfortunately, most of the drivers are not statically linked. This anyway lets you a chance to dynamically link the driver with the current kernel version, and try to make them work together.
+As we have explained before, manufacturers do release binary drivers in their GPL
+tarball. When those drivers are statically linked into the kernel, they become GPL
+as well, fortunately or unfortunately, most of the drivers are not statically linked.
+This anyway lets you a chance to dynamically link the driver with the current kernel
+version, and try to make them work together.
 
-This is one of the most tricky and grey part of the fully open source projects. Some drivers require few modifications to be working with your custom kernel, because they worked with an earlier kernel, and few modifications have been made to the kernel in-between those versions. This is for instance the case with the binary driver of the Broadcom BCM43xx Wireless Chipsets, where only few differences were made to the network interface structures.
+This is one of the most tricky and grey part of the fully open source projects. 
+Some drivers require few modifications to be working with your custom kernel, 
+because they worked with an earlier kernel, and few modifications have been made
+to the kernel in-between those versions. This is for instance the case with the 
+binary driver of the Broadcom BCM43xx Wireless Chipsets, where only few differences
+were made to the network interface structures.
 
-Some general principles can be applied no matter which kernel version is used in order to make binary drivers work with your custom kernel :
+Some general principles can be applied no matter which kernel version is used in
+order to make binary drivers work with your custom kernel:
 
 \begin{itemize}
-\item turn on kernel debugging features such as :
+\item turn on kernel debugging features such as:
 \begin{itemize}
 \item CONFIG\_DEBUG\_KERNEL
 \item CONFIG\_DETECT\_SOFTLOCKUP
 \item CONFIG\_DEBUG\_KOBJECT
-\item CONFIG\_EMBEDDED
 \item CONFIG\_KALLSYMS
 \item CONFIG\_KALLSYMS\_ALL
 \end{itemize}
@@ -180,31 +319,46 @@ Some general principles can be applied no matter which kernel version is used in
 \item catch the lockups and understand them
 \end{itemize}
 
-Most of the time, loading binary drivers will fail, and generate a kernel oops. You can know the last symbol the binary drivers attempted to use, and see in the kernel headers file, if you do not have to move some structures field before or after that symbol in order to keep compatibily with both the binary driver and the stock kernel drivers.
+Most of the time, loading binary drivers will fail, and generate a kernel oops. 
+You can know the last symbol the binary drivers attempted to use, and see in the
+kernel headers file, if you do not have to move some structures field before or 
+after that symbol in order to keep compatibily with both the binary driver and 
+the stock kernel drivers.
 
 \subsubsection{Understanding the firmware format}
 
-You might want to understand the firmware format, even if you are not yet capable of running a custom firmware on your device, because this is sometimes a blocking part of the flashing process.
+You might want to understand the firmware format, even if you are not yet capable
+of running a custom firmware on your device, because this is sometimes a blocking
+part of the flashing process.
 
-A firmare format is most of the time composed of the following fields :
+A firmware format is most of the time composed of the following fields:
 
 \begin{itemize}
-\item header, containing a firmare version and additionnal fields : Vendor, Hardware version ...
+\item header, containing a firmware version and additional fields: Vendor, Hardware version ...
 \item CRC32 checksum on either the whole file or just part of it
-\item Binary or compressed kernel image
-\item Binary or compressed root filesystem image
+\item Binary and/or compressed kernel image
+\item Binary and/or compressed root filesystem image
 \item potential garbage
 \end{itemize}
 
-Once you have figured out how the firmware format is partitionned, you will have to write your own tool that produces valid firmare binaries. One thing to be very careful here is the endianness of either the machine that produces the binary firmware and the device that will be flashed using this binary firmware.
+Once you have figured out how the firmware format is partitioned, you will have 
+to write your own tool that produces valid firmware binaries. One thing to be very
+careful here is the endianness of either the machine that produces the binary 
+firmware and the device that will be flashed using this binary firmware.
 
 \subsubsection{Writing a flash map driver}
 
-The flash map driver has an important role in making your custom firmware work because it is responsible of mapping the correct flash regions and associated rights to specific parts of the system such as : bootloader, kernel, user filesystem.
+The flash map driver has an important role in making your custom firmware work 
+because it is responsible of mapping the correct flash regions and associated 
+rights to specific parts of the system such as: bootloader, kernel, user filesystem.
 
-Writing your own flash map driver is not really a hard task once you know how your firmware image and flash is structured. You will find below a commented example that covers the case of the device where the bootloader can pass to the kernel its partition plan.
+Writing your own flash map driver is not really a hard task once you know how your
+firmware image and flash is structured. You will find below a commented example
+that covers the case of the device where the bootloader can pass to the kernel its partition plan.
 
-First of all, you need to make your flash map driver be visible in the kernel configuration options, this can be done by editing the file \textbf{linux/drivers/mtd/maps/Kconfig} :
+First of all, you need to make your flash map driver be visible in the kernel 
+configuration options, this can be done by editing the file \
+\textbf{linux/drivers/mtd/maps/Kconfig}:
 
 \begin{verbatim}
 config MTD_DEVICE_FLASH
@@ -215,16 +369,18 @@ config MTD_DEVICE_FLASH
          Bootloader Foo and Bootloader Bar.
 \end{verbatim}
 
-Then add your source file to the \textbf{linux/drivers/mtd/maps/Makefile}, so that it will be compiled along with the kernel.
+Then add your source file to the \textbf{linux/drivers/mtd/maps/Makefile}, so 
+that it will be compiled along with the kernel.
 
 \begin{verbatim}
 obj-\$(CONFIG_MTD_DEVICE_FLASH)      += device-flash.o
 \end{verbatim}
 
-You can then write the kernel driver itself, by creating a \textbf{linux/drivers/mtd/maps/device-flash.c} C source file.
+You can then write the kernel driver itself, by creating a 
+\textbf{linux/drivers/mtd/maps/device-flash.c} C source file.
 
 \begin{verbatim}
-// Includes that are required for the flash map driver to know of the prototypes :
+// Includes that are required for the flash map driver to know of the prototypes:
 #include <asm/io.h>
 #include <linux/init.h>
 #include <linux/kernel.h>
@@ -233,7 +389,7 @@ You can then write the kernel driver itself, by creating a \textbf{linux/drivers
 #include <linux/mtd/partitions.h>
 #include <linux/vmalloc.h>
 
-// Put some flash map definitions here :
+// Put some flash map definitions here:
 #define WINDOW_ADDR 0x1FC00000         /* Real address of the flash */
 #define WINDOW_SIZE 0x400000                /* Size of flash */
 #define BUSWIDTH 2                                   /* Buswidth */
@@ -262,7 +418,7 @@ static int __init device_mtd_init(void)
                return -EIO;
        }
 
-	   // Initlialise the device map
+	   // Initialize the device map
        simple_map_init(&device_map);
 
 	   /* MTD informations are closely linked to the flash map device
@@ -318,7 +474,117 @@ module_init(device_mtd_init);
 module_exit(device_mtd_cleanup);
 
 
-// Macros defining licence and author, parameters can be defined here too.
+// Macros defining license and author, parameters can be defined here too.
 MODULE_LICENSE("GPL");
 MODULE_AUTHOR("Me, myself and I <memyselfandi@domain.tld");
 \end{verbatim}
+
+\subsection{Adding your target in OpenWrt}
+
+Once you spotted the key changes that were made to the Linux kernel
+to support your target, you will want to create a target in OpenWrt
+for your hardware. This can be useful to benefit from the toolchain
+that OpenWrt builds as well as the resulting user-space and kernel
+configuration options.
+
+Provided that your target is already known to OpenWrt, it will be
+as simple as creating a \texttt{target/linux/board} directory
+where you will be creating the following directories and files.
+
+Here for example, is a \texttt{target/linux/board/Makefile}:
+
+\begin{Verbatim}[frame=single,numbers=left]
+#
+# Copyright (C) 2009 OpenWrt.org
+#
+# This is free software, licensed under the GNU General Public License v2.
+# See /LICENSE for more information.
+#
+include $(TOPDIR)/rules.mk
+
+ARCH:=mips
+BOARD:=board
+BOARDNAME:=Eval board
+FEATURES:=squashfs jffs2 pci usb
+
+LINUX_VERSION:=2.6.27.10
+
+include $(INCLUDE_DIR)/target.mk
+
+DEFAULT_PACKAGES += hostapd-mini
+
+define Target/Description
+        Build firmware images for Evaluation board
+endef
+
+$(eval $(call BuildTarget))
+\end{Verbatim}
+
+\begin{itemize}
+    \item \texttt{ARCH} \\
+        The name of the architecture known by Linux and uClibc
+    \item \texttt{BOARD} \\
+        The name of your board that will be used as a package and build directory identifier
+    \item \texttt{BOARDNAME} \\
+        Expanded name that will appear in menuconfig
+    \item \texttt{FEATURES} \\
+        Set of features to build filesystem images, USB, PCI, VIDEO kernel support
+    \item \texttt{LINUX\_VERSION} \\
+        Linux kernel version to use for this target
+    \item \texttt{DEFAULT\_PACKAGES} \\
+        Set of packages to be built by default
+\end{itemize}
+
+A partial kernel configuration which is either named \texttt{config-default} or which matches the kernel version \texttt{config-2.6.x} should be present in \texttt{target/linux/board/}.
+This kernel configuration will only contain the relevant symbols to support your target and can be changed using \texttt{make kernel\_menuconfig}.
+
+To patch the kernel sources with the patches required to support your hardware, you will have to drop them in \texttt{patches} or in \texttt{patches-2.6.x} if there are specific
+changes between kernel versions. Additionnaly, if you want to avoid creating a patch that will create files, you can put those files into \texttt{files} or \texttt{files-2.6.x}
+with the same directory structure that the kernel uses (e.g: drivers/mtd/maps, arch/mips ..).
+
+The build system will require you to create a \texttt{target/linux/board/image/Makefile}:
+
+\begin{Verbatim}[frame=single,numbers=left]
+#
+# Copyright (C) 2009 OpenWrt.org
+#
+# This is free software, licensed under the GNU General Public License v2.
+# See /LICENSE for more information.
+#
+include $(TOPDIR)/rules.mk
+include $(INCLUDE_DIR)/image.mk
+
+define Image/BuildKernel
+        cp $(KDIR)/vmlinux.elf $(BIN_DIR)/openwrt-$(BOARD)-vmlinux.elf
+        gzip -9 -c $(KDIR)/vmlinux > $(KDIR)/vmlinux.bin.gz
+        $(STAGING_DIR_HOST)/bin/lzma e $(KDIR)/vmlinux $(KDIR)/vmlinux.bin.l7
+        dd if=$(KDIR)/vmlinux.bin.l7 of=$(BIN_DIR)/openwrt-$(BOARD)-vmlinux.lzma bs=65536 conv=sync
+        dd if=$(KDIR)/vmlinux.bin.gz of=$(BIN_DIR)/openwrt-$(BOARD)-vmlinux.gz bs=65536 conv=sync
+endef
+
+define Image/Build/squashfs
+    $(call prepare_generic_squashfs,$(KDIR)/root.squashfs)
+endef
+
+define Image/Build
+        $(call Image/Build/$(1))
+        dd if=$(KDIR)/root.$(1) of=$(BIN_DIR)/openwrt-$(BOARD)-root.$(1) bs=128k conv=sync
+
+        -$(STAGING_DIR_HOST)/bin/mkfwimage \
+                -B XS2 -v XS2.ar2316.OpenWrt \
+                -k $(BIN_DIR)/openwrt-$(BOARD)-vmlinux.lzma \
+                -r $(BIN_DIR)/openwrt-$(BOARD)-root.$(1) \
+                -o $(BIN_DIR)/openwrt-$(BOARD)-ubnt2-$(1).bin
+endef
+
+$(eval $(call BuildImage))
+
+\end{Verbatim}
+
+\begin{itemize}
+    \item \texttt{Image/BuildKernel} \\
+        This template defines changes to be made to the ELF kernel file
+    \item \texttt{Image/Build} \\
+	This template defines the final changes to apply to the rootfs and kernel, either combined or separated
+	firmware creation tools can be called here as well.
+\end{itemize}
