X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/c4ce6af0a07a0ef041fcfd09125cc0557894722d..57cacb623bb9589a3f4a9e19d54a18da81516baa:/docs/network.tex

diff --git a/docs/network.tex b/docs/network.tex
index 7d811ba7f..df67eed71 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -31,6 +31,8 @@ packages.
 
 When using the \texttt{'static'} method like in the example, the  options \texttt{ipaddr} and
 \texttt{netmask} are mandatory, while \texttt{gateway} and \texttt{dns} are optional.
+You can specify more than one DNS server, separated with spaces.
+
 DHCP currently only accepts \texttt{ipaddr} (IP address to request from the server)
 and \texttt{hostname} (client hostname identify as) - both are optional.
 
@@ -102,3 +104,13 @@ As value it takes a list of ports with these optional suffixes:
 The CPU port defaults to tagged, all other ports to untagged.
 On Broadcom hardware the CPU port is always 5. The other ports may vary with
 different hardware.
+
+For instance, if you wish to have 3 vlans, like one 3-port switch, 1 port in a
+DMZ, and another one as your WAN interface, use the following configuration :
+
+\begin{Verbatim}
+config switch       "eth0"
+    option vlan0    "1 2 3 5*"
+    option vlan1    "0 5"
+    option vlan2    "4 5"
+\end{Verbatim}
