X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/d9219238b05cc37112dd11427581e1aa6b502b33..f39156a9a14b9a3c8b68b54bbb3306d1bf59a43f:/docs/network.tex?ds=sidebyside

diff --git a/docs/network.tex b/docs/network.tex
index 41febef8a..df67eed71 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -31,6 +31,8 @@ packages.
 
 When using the \texttt{'static'} method like in the example, the  options \texttt{ipaddr} and
 \texttt{netmask} are mandatory, while \texttt{gateway} and \texttt{dns} are optional.
+You can specify more than one DNS server, separated with spaces.
+
 DHCP currently only accepts \texttt{ipaddr} (IP address to request from the server)
 and \texttt{hostname} (client hostname identify as) - both are optional.
 
@@ -54,6 +56,24 @@ PPP based protocols (\texttt{pppoe}, \texttt{pptp}, ...) accept these options:
 
 For all protocol types, you can also specify the MTU by using the \texttt{mtu} option.
 
+\subsubsection{Setting up static routes}
+
+You can set up static routes for a specific interface that will be brought up 
+after the interface is configured.
+
+Simply add a config section like this:
+
+\begin{Verbatim}
+config route foo
+	option interface lan
+	option target 1.1.1.0
+	option netmask 255.255.255.0
+	option gateway 192.168.1.1
+\end{Verbatim}
+
+The name for the route section is optional, the \texttt{interface}, \texttt{target} and 
+\texttt{gateway} options are mandatory.
+Leaving out the \texttt{netmask} option will turn the route into a host route.
 
 \subsubsection{Setting up the switch (currently broadcom only)}
 
@@ -84,3 +104,13 @@ As value it takes a list of ports with these optional suffixes:
 The CPU port defaults to tagged, all other ports to untagged.
 On Broadcom hardware the CPU port is always 5. The other ports may vary with
 different hardware.
+
+For instance, if you wish to have 3 vlans, like one 3-port switch, 1 port in a
+DMZ, and another one as your WAN interface, use the following configuration :
+
+\begin{Verbatim}
+config switch       "eth0"
+    option vlan0    "1 2 3 5*"
+    option vlan1    "0 5"
+    option vlan2    "4 5"
+\end{Verbatim}
