X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/e5e9a3e92ef032924330fd42e42fa746efd093a6..0dd225201a15d54ac6a166185eb6b8a057ac846d:/docs/adding.tex

diff --git a/docs/adding.tex b/docs/adding.tex
index b1712ac9d..2b47e6a32 100644
--- a/docs/adding.tex
+++ b/docs/adding.tex
@@ -357,7 +357,7 @@ firmware image and flash is structured. You will find below a commented example
 that covers the case of the device where the bootloader can pass to the kernel its partition plan.
 
 First of all, you need to make your flash map driver be visible in the kernel 
-configuration options, this can be done by editing the file 
+configuration options, this can be done by editing the file \
 \textbf{linux/drivers/mtd/maps/Kconfig}:
 
 \begin{verbatim}
