X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/e64fdc9250243ee07a0f90c8e4204eff604446f5..11afdfa934dc20a1317d8414e779c11aaaf86e4e:/docs/network.tex

diff --git a/docs/network.tex b/docs/network.tex
index 2c65dd295..bb23fa524 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -115,6 +115,11 @@ config switch       "eth0"
     option vlan2    "4 5"
 \end{Verbatim}
 
+Three interfaces will be automatically created using this switch layout :
+\texttt{eth0.0} (vlan0), \texttt{eth0.1} (vlan1) and \texttt{eth0.2} (vlan2).
+You can then assign those interfaces to a custom network configuration name
+like \texttt{lan}, \texttt{wan} or \texttt{dmz} for instance.
+
 \subsubsection{Setting up IPv6 connectivity}
 
 OpenWrt supports IPv6 connectivity using PPP, Tunnel brokers or static
@@ -123,8 +128,9 @@ assignment.
 If you use PPP, IPv6 will be setup using IP6CP and there is nothing to
 configure.
 
-To setup an IPv6 tunnel to a tunnel broker, you have to edit the
-\texttt{/etc/config/6tunnel} file and change the settings accordingly :
+To setup an IPv6 tunnel to a tunnel broker, you can install the
+\texttt{6scripts} package and edit the \texttt{/etc/config/6tunnel}
+file and change the settings accordingly :
 
 \begin{Verbatim}
 config 6tunnel
@@ -151,6 +157,19 @@ config 6tunnel
 	IPv6 prefix to setup on the LAN.
 \end{itemize}
 
+Using the same package you can also setup an IPv6 bridged connection :
+
+\begin{Verbatim}
+config 6bridge
+	option bridge	'br6'
+\end{Verbatim}
+
+By default the script bridges the WAN interface with the LAN interface
+and uses ebtables to filter anything that is not IPv6 on the bridge.
+This configuration is particularly useful if your router is not
+IPv6 ND proxy capable (see: http://www.rfc-archive.org/getrfc.php?rfc=4389).
+
+
 IPv6 static addressing is also supported using a similar setup as
 IPv4 but with the \texttt{ip6} prefixing (when applicable).
 
@@ -159,4 +178,5 @@ config interface     "lan"
     option ifname    "eth0"
     option proto     "static"
     option ip6addr    "fe80::200:ff:fe00:0/64"
+    option ip6gw     "2001::DEAF:BEE:1"
 \end{Verbatim}
