X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/17d1b91a9611b9278c926e82c9be938ade02d095..2c05e6ab53215323d3f104e9cba8d50105ef9ef8:/docs/wireless.tex

diff --git a/docs/wireless.tex b/docs/wireless.tex
index 675023385..d6a71e28a 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -140,6 +140,14 @@ config wifi-iface
 	\item \texttt{mode} \\
 		The frequency band (\texttt{b}, \texttt{g}, \texttt{bg}, \texttt{a}). This feature is only supported on the atheros chipset.
 
+    \item \texttt{diversity} \\
+	Optional: Enable diversity for the Wi-Fi device. This feature is supported only on the atheros chipset.
+
+    \item \texttt{rxanteanna} \\
+	Optional: Antenna identifier (0, 1 or 2) for reception. This feature is supported only on the atheros chipset.
+
+    \item \texttt{txanteanna} \\
+	Optional: Antenna identifier (0, 1 or 2) for emission. This feature is supported only on the atheros chipset.
 
 \end{itemize}
 
