X-Git-Url: https://git.rohieb.name/openwrt.git/blobdiff_plain/4a834421b0600e62f0110302c0d50c52be0b282e..925c08e7b929c86e5753f716440c30f1c54c2c23:/docs/build.tex

diff --git a/docs/build.tex b/docs/build.tex
index fed0ca281..1335c8132 100644
--- a/docs/build.tex
+++ b/docs/build.tex
@@ -143,7 +143,15 @@ Similar to the linux kernel config, almost every option has three choices,
 \end{itemize}
 
 After you've finished with the menu configuration, exit and when prompted, save your
-configuration changes. To begin compiling the firmware, type "\texttt{make}". By default
+configuration changes.
+
+If you want, you can also modify the kernel config for the selected target system.
+simply run "\texttt{make kernel\_menuconfig}" and the build system will unpack the kernel sources
+(if necessary), run menuconfig inside of the kernel tree, and then copy the kernel config
+to \texttt{target/linux/\textit{<platform>}/config} so that it is preserved over
+"\texttt{make clean}" calls.
+
+To begin compiling the firmware, type "\texttt{make}". By default
 OpenWrt will only display a high level overview of the compile process and not each individual
 command.
 
